{
    "version": 1,
    "minor_version": 1,
    "key": "zwave_js.legacy_zwave_migration",
    "data": {
        "2a6df737202a830aa17b2829ed6ea9af": {
            "sensor.wallmote_quad_battery_level": {
                "node_id": 11,
                "endpoint_index": 0,
                "command_class": 128,
                "value_property_name": "level",
                "value_property_key_name": null,
                "value_id": "11-128-0-level",
                "device_id": "71e62180236f722599ae8befb018afaf",
                "domain": "sensor",
                "entity_id": "sensor.wallmote_quad_battery_level",
                "unique_id": "3487449463.11-128-0-level",
                "unit_of_measurement": "%"
            },
            "switch.z_wave_outdoor_smart_plug": {
                "node_id": 7,
                "endpoint_index": 0,
                "command_class": 37,
                "value_property_name": "currentValue",
                "value_property_key_name": null,
                "value_id": "7-37-0-currentValue",
                "device_id": "1534788968302894d63a9b69cfc31456",
                "domain": "switch",
                "entity_id": "switch.z_wave_outdoor_smart_plug",
                "unique_id": "3487449463.7-37-0-currentValue",
                "unit_of_measurement": null
            },
            "binary_sensor.wallmote_quad_power_management_battery_is_fully_charged": {
                "node_id": 11,
                "endpoint_index": 0,
                "command_class": 113,
                "value_property_name": "Power Management",
                "value_property_key_name": "Battery level status",
                "value_id": "11-113-0-Power Management-Battery level status",
                "device_id": "71e62180236f722599ae8befb018afaf",
                "domain": "binary_sensor",
                "entity_id": "binary_sensor.wallmote_quad_power_management_battery_is_fully_charged",
                "unique_id": "3487449463.11-113-0-Power Management-Battery level status.13",
                "unit_of_measurement": null
            },
            "binary_sensor.wallmote_quad_power_management_charge_battery_soon": {
                "node_id": 11,
                "endpoint_index": 0,
                "command_class": 113,
                "value_property_name": "Power Management",
                "value_property_key_name": "Battery level status",
                "value_id": "11-113-0-Power Management-Battery level status",
                "device_id": "71e62180236f722599ae8befb018afaf",
                "domain": "binary_sensor",
                "entity_id": "binary_sensor.wallmote_quad_power_management_charge_battery_soon",
                "unique_id": "3487449463.11-113-0-Power Management-Battery level status.14",
                "unit_of_measurement": null
            },
            "binary_sensor.wallmote_quad_power_management_charge_battery_now": {
                "node_id": 11,
                "endpoint_index": 0,
                "command_class": 113,
                "value_property_name": "Power Management",
                "value_property_key_name": "Battery level status",
                "value_id": "11-113-0-Power Management-Battery level status",
                "device_id": "71e62180236f722599ae8befb018afaf",
                "domain": "binary_sensor",
                "entity_id": "binary_sensor.wallmote_quad_power_management_charge_battery_now",
                "unique_id": "3487449463.11-113-0-Power Management-Battery level status.15",
                "unit_of_measurement": null
            },
            "binary_sensor.wallmote_quad_power_management_battery_is_charging": {
                "node_id": 11,
                "endpoint_index": 0,
                "command_class": 113,
                "value_property_name": "Power Management",
                "value_property_key_name": "Battery load status",
                "value_id": "11-113-0-Power Management-Battery load status",
                "device_id": "71e62180236f722599ae8befb018afaf",
                "domain": "binary_sensor",
                "entity_id": "binary_sensor.wallmote_quad_power_management_battery_is_charging",
                "unique_id": "3487449463.11-113-0-Power Management-Battery load status.12",
                "unit_of_measurement": null
            },
            "binary_sensor.wallmote_quad_low_battery_level": {
                "node_id": 11,
                "endpoint_index": 0,
                "command_class": 128,
                "value_property_name": "isLow",
                "value_property_key_name": null,
                "value_id": "11-128-0-isLow",
                "device_id": "71e62180236f722599ae8befb018afaf",
                "domain": "binary_sensor",
                "entity_id": "binary_sensor.wallmote_quad_low_battery_level",
                "unique_id": "3487449463.11-128-0-isLow",
                "unit_of_measurement": null
            }
        }
    }
}